**Sequential Optimization for Minimizing Material Cost and Treatment Time of Fenton Oxidation for Textile Wastewater Treatment**

Anam Asghar, Abdul Aziz Abdul Raman\*, Wan Mohd Ashri Wan Daud

1Postgraduate Student, Department of Chemical Engineering, Faculty of Engineering, University of Malaya, 50603 Kuala Lumpur, Malaysia. Email: chem.uet@hotmail.com

2Professor, Department of Chemical Engineering, Faculty of Engineering, University of Malaya, 50603 Kuala Lumpur, Malaysia. (Corresponding Author). Email: azizraman@um.edu.my

3Professor, Department of Chemical Engineering, Faculty of Engineering, University of Malaya, 50603 Kuala Lumpur, Malaysia. Email: ashri@um.edu.my

**SUPPLEMENTARY DATA**

**List of Tables**

Table S1 Experimental design matrix, experimental runs and predicted values on COD removal and Decolorization efficiency (Reprinted from Asghar et al., 2014).

Table S2 Optimized operating parameters (Reprinted from Asghar et al., 2014).

Table S3 L9 orthogonal design, Levels of four factors and experimental results obtained (Reproduced from main document of this paper).

Table S4 Fenton oxidation efficiency under optimized conditions

**List of Figures**

Figure S1. Mean S/N ratio for (a) COD (b) TOC removal

Figure S2. Mean S/N ratio for decolorization

**Central Composite Design**

Table S1 Experimental design matrix, experimental runs and predicted values on COD removal and Decolorization efficiency (Reprinted from Asghar et al., 2014).

|  |  |
| --- | --- |
| **Independent variables(X)** | **Dependent Variables (Y ;(%))** |
|  | **Actual values** | **Predicted Values** |
| **Run** | **Dye****(mg/L)** | **H2O2:Fe+2****(wt/wt)** | **Dye:Fe+2****(wt/wt)** | **pH** | **COD (%)** | **Decolorization (%)** | **COD (%)** | **Decolorization (%)** |
| **1** | 200 | 15 | 30 | 5.5 | 75.3 | 95.4 | 73.2 | 95.1 |
| **2** | 200 | 15 | 30 | 5.5 | 76.4 | 95.4 | 73.2 | 95.1 |
| **3** | 300 | 25 | 50 | 9 | 62.8 | 96.8 | 60.9 | 95.7 |
| **4** | 200 | 25 | 30 | 5.5 | 73.4 | 98.1 | 69.8 | 97.5 |
| **5** | 300 | 5 | 50 | 9 | 34.8 | 80.0 | 35.1 | 79.8 |
| **6** | 200 | 15 | 30 | 5.5 | 73.4 | 95.5 | 73.2 | 95.1 |
| **7** | 100 | 5 | 10 | 9 | 66.5 | 55.8 | 63.4 | 59.7 |
| **8** | 100 | 25 | 50 | 2 | 87.7 | 99.2 | 85.3 | 100.0 |
| **9** | 200 | 15 | 30 | 9 | 65.8 | 78.9 | 67.3 | 80.3 |
| **10** | 300 | 15 | 30 | 5.5 | 78.3 | 94.5 | 80.2 | 98.6 |
| **11** | 100 | 15 | 30 | 5.5 | 77.1 | 90.1 | 73.9 | 86.7 |
| **12** | 100 | 5 | 10 | 2 | 67.0 | 93.4 | 66.1 | 92.2 |
| **13** | 100 | 5 | 50 | 9 | 30.2 | 56.1 | 32.9 | 54.4 |
| **14** | 200 | 15 | 30 | 5.5 | 74.5 | 95.4 | 73.2 | 95.1 |
| **15** | 300 | 5 | 10 | 9 | 77.9 | 89.1 | 79.4 | 85.9 |
| **16** | 200 | 5 | 30 | 5.5 | 60.8 | 84.3 | 63.3 | 85.6 |
| **17** | 100 | 25 | 10 | 9 | 48.0 | 67.9 | 50.51 | 65.1 |
| **18** | 200 | 15 | 30 | 5.5 | 70.3 | 94.6 | 73.20 | 95.1 |
| **19** | 300 | 25 | 10 | 2 | 67.4 | 98.9 | 63.6 | 98.3 |
| **20** | 300 | 5 | 10 | 2 | 61.4 | 95.2 | 62.5 | 95.6 |
| **21** | 100 | 25 | 10 | 2 | 50.3 | 97.6 | 53.1 | 99.9 |
| **22** | 200 | 15 | 10 | 5.5 | 67.7 | 98.2 | 67.7 | 97.7 |
| **23** | 300 | 25 | 10 | 9 | 80.4 | 84.4 | 80.5 | 86.3 |
| **24** | 300 | 25 | 50 | 2 | 75.5 | 99.4 | 81.8 | 97.7 |
| **25** | 200 | 15 | 30 | 2 | 74.1 | 98.3 | 79.1 | 97.5 |
| **26** | 100 | 25 | 50 | 9 | 44.7 | 73.6 | 44.9 | 75.4 |
| **27** | 200 | 15 | 50 | 5.5 | 62.7 | 93.5 | 61.6 | 94.7 |
| **28** | 200 | 15 | 30 | 5.5 | 73.4 | 96.6 | 73.2 | 95.1 |
| **29** | 100 | 5 | 50 | 2 | 72.1 | 76.5 | 73.4 | 76.7 |
| **30** | 300 | 5 | 50 | 2 | 61.2 | 78.9 | 55.9 | 79.4 |

Table S2 Optimized operating parameters (Reprinted from Asghar et al., 2014).

|  |  |
| --- | --- |
|  |  Predicted responses |
| Dye(mg/L) | **Dye: Fe+2****(wt/wt)** | **H2O2:Fe+2****(wt/wt)** | **pH** | **COD (%)** | **Decolorization (%)** | **Desirability** |
| 300 | 25.92 | 19.15 | 3 | 81.64 | 99.40 | 0.972 |

**Taguchi Method**

Table S3 L9 orthogonal design, Levels of four factors and experimental results obtained (Reproduced from main document of this paper)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Runs**  | **Dye** | **Dye:Fe+2** | **H2O2:Fe+2** | **pH** | **COD** | **TOC** | **Decolorization** |
|  | **mg/L** | **wt/wt** | **wt/wt** |  | **(%)** | **(%)** | **(%)** |
| **1** | 1 | 1 | 1 | 1 | 77.01 | 63.17 | 98.86 |
| **2** | 1 | 2 | 2 | 2 | 35.63 | 30.16 | 96.67 |
| **3** | 1 | 3 | 3 | 3 | 16.09 | 9.93 | 96.96 |
| **4** | 2 | 1 | 2 | 3 | 14.29 | 5.48 | 91.42 |
| **5** | 2 | 2 | 3 | 1 | 80.13 | 72.86 | 96.99 |
| **6** | 2 | 3 | 1 | 2 | 46.75 | 46.75 | 96.25 |
| **7** | 3 | 1 | 3 | 2 | 30.60 | 41.44 | 99.31 |
| **8** | 3 | 2 | 1 | 3 | 7.65 | 12.35 | 93.12 |
| **9** | 3 | 3 | 2 | 1 | 66.56 | 59.02 | 99.60 |

Table S4 Fenton oxidation efficiency under optimized conditions

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Parameter | Dye | Dye:Fe+2 | H2O2: Fe+2 | pH | Predicted |
| COD | 200 | 50 | 25 | 3 | 76.29 |
| TOC | 300 | 50 | 5 | 3 | 66.297 |
| Decolorization | 100 | 50 | 25 | 3 | 98.51 |

\*Experiments on Taguchi were not performed. And Taguchi optimization technique was extended to do approximate cost estimations





Figure S1. Mean S/N ratio for **(a)** COD **(b)** TOC removal



Figure S2. Mean S/N ratio for decolorization

**References**

Asghar, A., Abdul Raman, A.A. and Daud, W. M. A. W. (2014). A Comparison of Central Composite Design and Taguchi Method for Optimizing Fenton Process. *Sci. World J.,* 2014(2014), 14.