
**Petroleum generation and migration in the Cambro-Ordovician Laurentian margin succession of NW Scotland**

**J. PARNELL, S. BOWDEN & D. MARK**

**Supplementary Material (dataset)**

Technical Data



All samples were irradiated in the OSU CLICIT reactor.

Sample standard = GA1550 @ 99.738 ± 0.104 Ma (Renne et al., 2011), equivalent to FCs @ 28.294 Ma

Sample Reference Duration (minutes)

JP Cambrian Quartzite EK56 3600

Raw results

